**AQUAPANEL® Cement Board Indoor (Lighter. Easier. Faster.)**

#### Skim coat above the tile level in Q4 quality

|  |
| --- |
| Specification examples |

# 

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Item | Quantity / ME | Description of service | Unit cost | Total cost |
|  | m²  m²  m² | **Wall lining with cement-bonded building boards, primed all-over, AQUAPANEL® Q4-finish above the tile level**  Above the tile level all visible joints should be covered with AQUAPANEL® Q4- Finish, Knauf fibreglass joint covering strips are to be pressed into the skim coat, apply another thin layer of AQUAPANEL® Q4- Finish to the cover strips, remove residues.  Cover all screw heads.  When dry, remove irregularities on the surface and screw holes with a hand grinder.  Apply another layer of AQUAPANEL® Q4-Finish in a width of at least 20cm onto the existing layer in the joint area.  Sand off irregularities again when dry.  All-over skim coat of AQUAPANEL® Q4-Finish above the tile level.  After drying and interim sanding if necessary, apply a further layer of AQUAPANEL® Q4-Finish.  After approx. 24 h drying, the surface can be sanded with sanding  paper (grain 120). Very smooth surfaces can be achieved, e.g. with an electric orbital sander.  Comment:  Height Tile level  > Height Area smoothed with AQUAPANEL® Q4-Finish  Perform all work according to manufacturer's instructions. |  |  |